Model: PBS-11

Type: self-locking/non-locking

Current: 11A

Material of conductor: copper foot

Opening Diameter: 12MM

Rated current: 3A

Rated voltage:250V

Foot width:3M Thickness 0.5MM

Length:32.7MM Total length:38.8MM

Main technical parameters：

|  |  |
| --- | --- |
| Rated Voltage/Current | 3A250VAC/6A125VAC |
| Dielectric strength | 1500VAC/1min |
| Insulation resistance | >100mΩ |
| Contact resistance | <50mΩ |
| Electrical life | 10000 times |
| Ambient Temperature | -40~+85℃ |