
**Electric Tricycle Brushless Differential Motor 1500W 3000W**



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Rated Power** | 1500W | 2200W | 3000W | 3000W |
| **Rated volt** | 60V/72V | 60V/72V | 60V | 72V |
| **Rated Speed** | 3200 | 60/72V | 60V | 72V |
| **Rated Current**  **(A)** | ≤31-28 | ≤43-39 | ≤58 | ≤58 |
| **Rated torque** | 6.2n.m | 8.2n.m | 10.1n.m | 10.1n.m |
| **Rated Effeciency** | 83% | 83% | 83% | 83% |
| **Application range** | Middle&Heavy electric tricycle | | | |



